Step 1. Print the pattern out and past it on a large kraft.
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Step 2: Cut off the kraft, you will get the template to be used.
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Step3: Oil the leather that you will use. After that, don’t forget to dry it by an air dryer.
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Step 4: Paint leather treatment on the flesh side, smooth with a piece of glass board, and dry it with an air dryer.
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Step 5: When dried, you can use the polish stick to smooth the flesh side, to get a perfect smooth effect.
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Step 6: Now you can paint leather coat on the surface side and dry it. The surface becomes shining and anti-water now.
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Step 7: After the steps above we can begin to make. First draw outlines according to the patterns on leather..
[image: image13.jpg]


[image: image14.jpg]



Step 8: Cut off the drew pieces with scissors and knife.
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Step 9: Iron the edge to make it smooth and draw a decoration line by hot edge line drawer. Both the tools you can buy from 
https://www.etsy.com/shop/LZpattern?section_id=14631840&ref=shopsection_leftnav_4
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Step 10: Bevele the edge by a beveler. You can also buy this tools from our shop.
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Step 11: Sew the upside.
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And don’t forget to shew the bottom of the card slots. Each one should be sewed.
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Step 12: Bevele the other edges.
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Step 13: Stick a piece of fabric on a piece of 0.5mm pig skin.
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Step 14: Pierce holes on the stitch anchor points to make marks on leather with your awl.
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Step 15: You can punch holes and sew then together now. After sewing, cut off the redundant part
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Step 16: Paste the strap on and pierce stitch marks.
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Step 17: After sew left part, you can go on to pierce marks and punch holes. You can add a layer of pig skin as lining for the strap, here I didn’t do it.
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Step 18: Paste a same large pig skin on to hide everying in.
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Step 19: Sew the beam leather on.
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Step 20: Finally, sew the inner construction on the Surface, finish this work.
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