General Quick Start Guide
[bookmark: _GoBack]Notes and Tips:
· IMPORTANT! If you resize the pattern, note that the buckle is designed for a set 2” width so if you wish to keep the buckle at 2”, print the strap pattern first at normal scale, then print out a scaled up or down version to your preference and compensate for the different hole placements.  The buckle can also be resized to accommodate a different sized buckle if you wish.
· When printing the patterns make sure you find the option to ‘Print actual size’ otherwise the faceplate may be scaled down slightly to fit on the page.
· The pattern is sized for roughly medium to lg but
· To ensure a preferred fit, cut out all the pattern pieces and construct a paper mockup first by taping it together.  The paper lacks the dimensions of leather so if it fits snug as paper, definitely scale it up slightly.  Your printing device and PDF viewing software may vary so Google search “how to scale pdf printing” if you’re having trouble with this.
· On the pattern piece that requires multiple tracings you may wish to use some light adhesive to glue the pattern to some card stock or thin cardboard backing.  
· I designed this to be a fairly straightforward design so feel free to experiment with the design to make it your own.
· Be sure to share your results with us! Tag PrinceArmory on any of the social networks or share it on one of our pages.
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